# Producted Water Treatment

#### Produced Water Treatment

#### Crude and Produced Water Equipment

- We have a integrated system in place that shall reduce water quality to 30ppm and below to meet client’s and regulatory bodies standard specification.
- All approvals shall be sought from regulatory agenciesi.e NUPRC, Navy, Nimasa
- Treated produced water formation shall be barged to an appriopriate approved water disposal area according to the regulation (200m and 12 Northical miles from the shore)
- Evaluation of geophysical, geological, core, log, PVT, well test , production and pressure data to determine hydrocarbons-in-place, estimate recoverable reserves, production profiles and ultimately, production enhancement
- Self propelled Fit for purpose vessel for Crude evacuation duly approved vessel coastal licence with all safety aparatus: fenders, fire and thunder arrestors etc

#### Equipment Categories

- Single stanby 100,000BBl caliberated Barge to receive crude from process facility.
- Two Calibrated Crude shuttle tankers of 18000BBl (depending on Tenoil daily production)
- 2 Produced water shuttle barges making a 18-24hrs round trip
- Telor made hose and sizable pumps shall be deployed

Join Our Team

### Maxupstream Energy Service Limited Is Waiting For You To Build An Inspirational Career

Are you looking for a reputable company to build up your carrer in oil & Gas? Click on the apply button to check for openings.

Apply Now

© Maxupstream Energy Service Limited Design by Buzydev